The kit includes:

profiled solid pine or spruce walls 34mm thick

20mm thick floor board

solid roof decking 20mm thick

foundation beams coated with an antiseptic solution to prevent rotting

enough nails and screws to assemble the house

details, drawings and assembly instructions.