The kit includes:

profiled solid pine or spruce walls 34mm thick

double door

two windows

20mm thick floor board

solid roof decking 20mm thick

foundation beams coated with an antiseptic solution to prevent rotting

enough nails and screws to assemble the house

door and window hardware kits

details, drawings and assembly instructions.

At the request of the customer, the double-leaf door can be both deaf and glazed.